PRETREATMENT RATIONALE FOR REISSUANCE – PUBLIC NOTICE DRAFT

Weyerhaeuser NR Company, Bruce Facility    	Permit No.: MSP092455
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Calhoun County            
Bruce, Mississippi  
Water II Branch    
  
SIC Code: 2421    
Permit Writer: Carter Cress 
August 19, 2026  
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I. FACILITY INFORMATION

1. Nature of Business: Lumber mill.            
1. Process Wastewater Description: Continuous discharge of kiln condensate.    
1. Proposed Flowrate:	Outfall 001: 0.050 MGD Monthly Avg. and Report Daily Max. 
D.	Applicable Federal Guidelines: 40 CFR Part 429 – Timber Products Processing Point Source Category; Subpart K – Sawmills and Planing Mills Subcategory.  Specifically, 40 CFR 429.125 – Pretreatment Standards for Existing Sources (PSES).     
E.	Process Wastewater Treatment: Oil/water separator thence an aerated lagoon.       

II. RECEIVING POTW INFORMATION

1. POTW Name, AI No., and Permit No.: Bruce POTW, 13040, MS0042129           
1. POTW Treatment Type: Aerated lagoon system followed by chlorine disinfection.    
1. POTW Design Flowrate: November – April: 0.50 MGD Maximum Monthly Average    
        May – October: 0.337 MGD Maximum Monthly Average    
1. POTW Receiving Stream: Skuna River                   
1. POTW Receiving Stream 7Q10 (Q7/10): 2.48 cfs = 1.60 MGD          

POTW Maximum Monthly Average flowrates in Million Gallons per Day (MGD) on year 2025 annual DMR: 

	November – April
	May – October 

	0.314
	0.142



      POTW 12-month Average Flow for year 2025 (QPOTW): 0.228 MGD

III.    CATEGORICAL REGULATIONS    

40 CFR Part 429 – Timber Products Processing Point Source Category; Subpart K – Sawmills and Planing Mills Subcategory.  Specifically, 40 CFR 429.125 – Pretreatment Standards for Existing Sources (PSES).  

Any existing source subject to this subpart which introduces process wastewater pollutants into a publicly owned treatment works must comply with 40 CFR Part 403 – General Pretreatment Regulations for Existing and New Sources of Pollution.  [40 CFR 429.125]  

IV.	DATA FROM FORM 2-P PERMIT APPLICATION 


	Outfall 001

	Pollutant 
	Long-term Average Value
	Maximum Daily Value

	Flow
	0.03 MGD
	0.09 MGD

	BOD
	23.62 mg/L
	86.0 mg/L

	Total Suspended Solids
	88.23 mg/L
	330.0 mg/L

	Oil and Grease
	0.23 mg/L
	5.0 mg/L

	pH
	6.4 SU (minimum)
	7.3 SU (maximum)

	COD
	---
	1,340 mg/L

	Ammonia (as N)
	---
	< 0.0539 mg/L




V.	DATA FROM DISCHARGE MONITORING REPORTS (DMRS)


	Outfall 001

	Parameter 
	Year 2023
	Year 2024
	Year 2025
	Year 2026* 

	Largest Average Flow
	0.0436 MGD
	0.0468 MGD
	0.049 MGD
	0.04 MGD

	Largest Maximum Flow
	0.078 MGD
	0.1172 MGD
	0.087 MGD
	0.087 MGD

	Largest Average BOD5
	276 mg/L
	110 mg/L
	140 mg/L
	40.1 mg/L

	Largest Maximum BOD5
	510 mg/L
	150 mg/L
	160 mg/L
	78 mg/L

	Largest Average TSS
	365 mg/L
	295 mg/L
	450 mg/L
	174 mg/L

	Largest Maximum TSS
	500 mg/L
	410 mg/L
	670 mg/L
	330 mg/L

	Largest Average O&G
	110.5 mg/L
	NODI=B1
	3 mg/L
	NODI=B

	Largest Maximum O&G
	221 mg/L
	NODI=B
	5.4 mg/L
	NODI=B

	Smallest Minimum pH
	6.5 SU
	6.5 SU
	6.4 SU
	6.5 SU

	Largest Maximum pH
	7.1 SU
	7.4 SU
	7.2 SU
	7.1 SU


   
   	*through April 

     	1 NODI=B is an EPA indicator code that means “below detection limit/no detection.”
	 
   	Please note: bold values indicate violations of current permit limits.  No violations were reported.  

VI.	PROPOSED PERMIT LIMITATIONS – OUTFALL 001

	Parameter
	Categorical Limits
(CAT)
	Current Permit Limits 
(CPL)
	Proposed Permit Limits 
(PPL)
	Sampling Frequency
	Sample Type
	Basis of Decision

	
	Avg.
lb/day

	Max.
lb/day

	Avg.
mg/L
	Max.
mg/L
	Avg.
lb/day
	Max.
lb/day
	Avg.
mg/L
	Max.
mg/L
	Avg.
lb/day
	Max.
lb/day
	Avg.
mg/L
	Max.
mg/L
	
	
	

	BOD5
	---
	---
	---
	---
	Report
	Report
	Report
	Report
	Report
	Report
	Report
	Report
	Once per Month
	Grab
	CPL

	TSS
	---
	---
	---
	---
	Report
	Report
	Report
	Report
	Report
	Report
	Report
	Report
	Once per Month
	Grab
	CPL

	Oil and Grease
	---
	---
	---
	---
	Report
	Report
	Report
	Report
	Report
	Report
	Report
	Report
	Once per Month
	Grab
	CPL



	 Parameter
	Categorical Limits
(CAT)
	Current Permit Limits 
(CPL)
	Proposed Permit Limits 
(PPL)
	Sampling 
Frequency
	Sample 
Type
	Basis of 
Decision

	
	Avg.
	Max.
	Avg.
	Max.
	Avg.
	Max.
	
	
	

	Flow
	---
	---
	0.050 MGD
	Report MGD
	0.050 MGD
	Report MGD
	Daily 
	Totalizer 
	CPL

	pH
	5.0 SU (min.)
	---
	5.0 SU (min.)
	9.0 SU
	5.0 SU (min.)
	9.0 SU
	Once per Month
	Grab 
	CPL



The monitoring analyses for BOD5, TSS, oil and grease, flow, and pH shall be submitted on a monthly DMR.  

VII.   STATEMENT OF BASIS (narrative)

In a cover letter to the permit application, the facility has requested changes to its monitoring requirements.  The facility requests that the sampling frequency for BOD5, TSS, oil and grease, and pH be reduced from twice per month to once per month.  Additionally, the facility requests that the sample type for BOD5 and TSS be changed from 24-hour composite to grab.     

A facility search found two other Weyerhaeuser lumber mills that discharge treated kiln condensate to the local POTWs.  Accordingly, these two facilities possess active water pretreatment permits.  These two facilities are Weyerhaeuser NR Company, McComb Wood Products and Weyerhaeuser NR Company, Philadelphia Facility.  Both of them require once per month sampling of BOD5, TSS, oil and grease, and pH.  Also, both require grab sampling for BOD5 and TSS.  Since no specific concerns were revealed for Weyerhaeuser NR Company, Bruce Facility, the aforementioned requested changes to its monitoring requirements have been granted.          

A public notice will be required for this permit reissuance.  
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