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PERMIT REVIEW SUMMARY

Permit Writer:	Ryan Wigginton 	Date:	May 10, 2026
Company Name:	KDM Custom Coatings Inc
Facility Location:	1989 Royal Maid Drive
Source Number:	1540-00138
County: 		Lee

FACILITY DESCRIPTION
KDM Customs, LLC (KDM), operates a synthetic minor operating source in Tupelo, Mississippi.  The facility’s operations fall under SIC code 3479: Coating, Engraving, and Allied Services, Not Elsewhere Classified and NAICS code 332812: Metal Coatings, Engravings (except Jewelry and Silverware), and Allied Services to Manufacturers.  
Surface coating operations (Emission Point AA-100) involve utilizing spray guns to apply powder coats electrostatically to metal parts.  The parts are then placed inside electric curing ovens.  This emission source also includes engineered coating processes and an HVAF coating system (equipped with a dust collection system).  Abrasive blasting operations (Emission Point AB-100) is used to smooth and clean unfinished metal parts.  This system is equipped with a cartridge filter dust collector system.  Propane is combusted (Emission Point AC-100) in the chamber of the spray guns to heat the coatings.  Welding operations (Emission Point AD-100) are performed occasionally to spot weld for repair metal components.
PROJECT/PERMIT ACTION DESCRIPTION
KDM has applied for reissuance of the Synthetic Minor Operating Permit (SMOP) No. 1540-00138.  The only change requested for this permitting action was removal of the concrete truck coating operation from Emission Point AA-100, as this was only practiced for a short time before being discontinued.  Some minor changes were incorporated into the permit to modernize it to current air permitting practices.
EMISSION SUMMARY
	Pollutant
	Facility-Wide Emission Rate (tons/yr)

	PM/PM10/PM2.5
	95.01

	VOC
	95.01

	Individual HAP
	9.902

	Total HAP
	24.902

	Sulfur Dioxide (SO2)
	0.0

	Nitrogen Oxides (NOX)
	0.01

	Carbon Monoxide (CO)
	0.00


1Facility-wide emission limits to remain below Title V threshold.
2Facility-wide emission limits to remain below HAP major source threshold.

APPLICABLE/PROPOSED PERMIT LIMITATIONS
Process equipment at the site has the potential to emit more than the Title V threshold (100 tons per year) of particulate matter (PM) and volatile organic compounds (VOC).  KDM also has the potential to emit more than the hazardous air pollutant (HAP) major source threshold of 25 tons per year (tpy) of total HAP and 10 tpy of individual HAP.  KDM has chosen to take synthetic minor limitations for each to remain below the Title V and HAP major source thresholds.  
	Emission Point
	Applicable Requirement
	Pollutant/ Parameter
	Limitation/Standard
	Monitoring/Recordkeeping/ Reporting Requirement

	AA-000 (Facility-Wide)
	11 Miss. Admin. Code Pt. 2, R. 1.3.A.
	Opacity
	≤ 40%
	Operate and maintain dust collectors in accordance with manufacturer’s specifications.  Maintain a log of maintenance.

	
	11 Miss. Admin. Code Pt. 2, R. 1.3.B.
	
	≤ 40%
	

	
	11 Miss. Admin. Code Pt. 2, R. 1.3F(1).
	PM (filterable only)
	E = 4.1 × p0.67
	

	
	11 Miss. Admin. Code Pt. 2, R. 2.2.B(10)., as established in Permit to Construct issued December 5, 2014
(Title V Avoidance Limit)
	PM/PM10 (filterable only)
	≤ 95.0 tpy
	Monitor and record abrasive blasting amount used and hours of operation and the amount of coating used and the hours of operation. Report facility wide PM emissions.

	
	11 Miss. Admin. Code Pt. 2, R. 2.2.B(10)., as established in Permit to Construct issued December 5, 2014
(Title V Avoidance Limit)
	VOC
	≤ 95.0 tpy
	Monitor and record VOC and HAP containing material used. Report facility wide VOC and HAP emissions.

	
	11 Miss. Admin. Code Pt. 2, R. 2.2.B(10)., as established in Permit to Construct issued December 5, 2014
(Major Source Avoidance Limits)
	HAP
	≤ 24.90 tpy total HAP
≤ 9.90 tpy individual HAP
	

	AC-100
	11 Miss. Admin. Code Pt. 2, R. 1.3.D(1)(a).
	PM
	≤ 0.6 lb/MMBtu-hr
	Margin of compliance is large; therefore, no monitoring requirements are incorporated into this permitting action.

	
	11 Miss. Admin. Code Pt. 2, R. 1.4.A(1).
	SO2
	≤ 4.8 lb/MMBtu-hr
	


NSPS APPLICABILITY
40 CFR 60, Subpart TT – Standards of Performance for Metal Coil Surface Coating:  this subpart applies to facilities that engage in metal coil surface coating operation.  KDM does not coat coils; therefore, this subpart does not apply.
MACT APPLICABILITY
40 CFR 63, Subpart MMMM – National Emission Standards for Hazardous Air Pollutants for Surface Coating of Miscellaneous Metal Parts and Products:  This subpart applies to major sources of HAP.  KDM has taken emission limits to remain an area source of HAP; therefore, this subpart does not apply.

40 CFR 63, Subpart HHHHHH – National Emission Standards for Hazardous Air Pollutants for Paint Stripping and Miscellaneous Surface Coating Operations at Area Sources:  This subpart applies to equipment used to apply surface coating to miscellaneous parts made of metal or plastic.  The target HAPs of this subpart are chromium, lead, manganese, nickel, and/or cadmium.  The coatings at KDM do not contain these target HAPs.  Additionally, 63.11180, “spray-applied coatings” excludes thermal spray operations; therefore, this subpart does not apply.

40 CFR 63, Subpart XXXXXX – National Emission Standards for Hazardous Air Pollutants for Nine Metal Fabrication and Finishing Source Categories:  This subpart applies to a particular list of SIC codes.  KDM’s operations do not fall under one of the listed source categories; therefore, this subpart does not apply.


PUBLIC PARTICIPATION

The 30-day public notice period began on July 22, 2026, when the notice was posted on MDEQ’s website and ends August 24, 2026.
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