PUBLIC NOTICE PERMIT RATIONALE FOR REISSUANCE
Fred Netterville Lumber Company
Wilkinson County
Woodville, Mississippi
Water NPDES No. MS0048577
July 13, 2026

I. FACILITY INFORMATION

Facility Name:		Fred Netterville Lumber Company
Facility Address:	3975 Buffalo Road 
	Woodville, MS 39669    
Woodville, 
Permit No.:		MS0048577
SIC:			2421
Permit Writer:		Rusty Parrish
EPD Branch: 		Water II Branch

II. NATURE OF BUSINESS

Fred Netterville Lumber Company converts hardwood logs into lumber. Processes at the facility include de-barking, sawing, planing selected pieces, and kiln drying. As of May 6, 2026, operations at the facility are not occurring but plans to resume operations in the future.

III. EFFLUENT AND RECEIVING STREAM FLOW DATA

When operating, existing Outfall 002 discharges approximately 500 gallons per day of boiler blowdown mixed with stormwater into a sedimentation basin. Discharge from the sedimentation basin is rainfall dependent, and the receiving stream is an unnamed tributary of Buffalo River.

IV. 303(d) and TOTAL MAXIMUM DAILY LOAD (TMDL) ISSUES

Buffalo River does appear on the Mississippi 2024 List of Impaired Water Bodies for sediment. The facility complies with the following applicable TMDL:
· Sediment – Designated Streams in the South Independed Streams Basin – March 2009 – ID: 609032501

V. TYPE OF WASTEWATER TREATMENT

Sedimentation via sedimentation basin. The discharge from existing Outfall 002 is rainfall dependent and does not occur as part of normal operations at the facility.

VI. EPA APPLICABLE CATEGORICAL GUIDELINES

40 CFR Part 429 – Timber Products Processing Point Source Category, Subpart K – Sawmills and Planing Mills Subcategory, specifically 429.123.

VII.	DATA FROM APPLICATION FORM 2C

The facility has not been in operation, so effluent from Outfall 002 was not able to be sampled. Historical data from the 2019 application was used in the following table to be a representative sample of the Outfall 002 effluent.

	Parameter
	Maximum Daily Value

	BOD
	26 mg/l

	COD
	187 mg/l 

	TOC
	53.3 mg/l

	TSS
	28 mg/l

	Ammonia
	ND

	pH 
	6.8 s.u.

	Temperature (Summer)
	33℃ = 91.4 deg F

	Oil & Grease
	2.2 mg/L



PROPOSED FINAL LIMITATIONS 

1. Average Permit Limitations: Outfall 002

	Parameter
	Categorical Limitation
	Water Quality
Limitation
	Current Permit Limitation
	Proposed Permit Limitation
	Basis

	pH
	-----
	6.0 SU (min)
	6.0 SU (min)
	6.0 SU (min)
	MSWQS

	Flow
	-----
	-----
	Report MGD
	Report MGD
	CPL

	Temperature
	-----
	-----
	-----
	-----
	-----



2. Maximum Permit Limitations: Outfall 002

	Parameter
	Categorical Limitation
	Water Quality
Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	Basis

	pH
	-----
	9.0 SU (max)
	9.0 SU (max)
	9.0 SU (max)
	MSWQS

	Flow
	-----
	-----
	Report MGD
	Report MGD
	CPL

	Temperature
	-----
	-----
	90 degrees F
	90 degrees F
	MSWQS


	MSWQS = Mississippi Water Quality Standard; CPL = Current Permit Limit

pH and Temperature shall be monitored quarterly via grab sampling. Flow shall be monitored quarterly via instantaneous sampling. 

One special condition of the permit as per 40 CFR Part 429, Subpart K, shall be that there shall be no discharge of process wastewater from the sedimentation basin. Another special condition of the permit shall be that there shall be no discharge from the vehicle washing operation.  

The existing permit contains a condition which requires no discharge of debris.  This condition is applicable to the log spray operation at the site. The log spraying operation is covered under the State of Mississippi Wet Decking General Permit which also contains this condition.
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