PERMIT RATIONALE FOR REISSUANCE
Transcontinental Gas Pipeline Company LLC, Station 70
Walthall County
Tylertown, Mississippi
Water NPDES No. MS0038482
July 16, 2026

I. FACILITY INFORMATION

Facility Name: 	Transcontinental Gas Pipeline Company LLC, Station 70
Facility Address: 	967 Highway 583 
	Tylertown, MS  39667    
Walthall, 
Permit No.: 		MS0038482
SIC: 			4922
Permit Writer:  	Tye Gardner
EPD Branch:  		Water I Branch

II. NATURE OF BUSINESS

Natural gas transmission. The facility is classified as an NPDES minor source.

III. EFFLUENT AND RECEIVING STREAM FLOW DATA

Outfall 001: Existing outfall consisting of floor drains and storm water. The facility previously discharged cooling tower blowdown, boiler blowdown, and reverse osmosis backwash, but that equipment has been isolated and placed out of service as stated in the April 2026 renewal application. The outfall would discharge into an Unnamed Tributary of Leatherwood Creek. 

The 7Q10 flow of Leatherwood Creek is 0.9 cfs (0.5186 MGD) and the Mean Annual Flow is 12.7 cfs (8.208 MGD).  Leatherwood Creek is classified and “Fish and Wildlife” and the Bogue Chitto River is classified as “Recreational”. Both streams are located in the Pearl River Basin.


IV. 303(d) and TOTAL MAXIMUM DAILY LOAD (TMDL) ISSUES

Leatherwood Creek does not appear on the 2026 303(d) List of Impaired Water Bodies. 
The facility complies with the following applicable TMDLs: 
· Fecal Coliform – Bogue Chitto River – Lawrence, Lincoln, Pike, and Walthall Counties – May 2000 – ID: 500051602 
· Fecal Coliform – Pearl River – Hancock County – December 2000 – ID: 500121503 
· Low pH – Pearl River – Neshoba, Leake, Hinds, Rankin, and Hancock Counties – December 2000 – ID: 500121501 

· Mercury – Bogue Chitto River – Lincoln, Pike, and Walthall Counties – December 2000 – ID: 500121501
· Sediment – Pearl River Basin – March 25, 2009 – ID: 509032501 
· Total Nitrogen and Total Phosphorus – Pearl River – Pearl River Basin – June 29, 2009 


V. TYPE OF WASTEWATER TREATMENT

None according to April 2026 application.

VI. EPA APPLICABLE CATEGORICAL GUIDELINES

Not Applicable.

VII.	DATA FROM APPLICATION FORM (2C)

According to April 2026 application, the facility has not discharged in approximately 6 years. Therefore, no data is available for this facility.

VIII. 	WATER QUALITY LIMITATIONS BASED ON WASTELOAD ALLOCATION 

	None.

1. CATEGORICAL GUIDELINE LIMITATIONS CALCULATIONS

Not Applicable.

TOXICITY SCREENING

Not Applicable.

XI.	PROPOSED FINAL LIMITATIONS 

1. Average Permit Limitations

	Outfall
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	1Basis

	001
	Flow (MGD)
	---
	---
	Report
	Report
	PPL, TJ

	001
	pH (min)
	---
	6.0 SU
	6.0 SU
	6.0 SU
	PPL, MSWQS

	001
	Oil and Grease
	---
	---
	10 mg/L
	10 mg/L
	PPL, TBEL

	001
	BOD5
	---
	---
	Report
	Report
	PPL, TJ

	001
	Zinc, Total Recoverable
	---
	0.065 mg/L
	0.0581 mg/L
	0.0581 mg/L
	PPL, TJ

	001
	TSS
	---
	---
	30 mg/L
	30 mg/L
	PPL, TJ

	001
	Ammonia (as N)
	---
	---
	Report
	Report
	PPL, TJ






2. Maximum Permit Limitations

	Outfall
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	1Basis

	001
	Flow (MGD)
	---
	---
	Report
	Report
	PPL, TJ

	001
	pH (min)
	---
	9.0 SU
	9.0 SU
	9.0 SU
	PPL, MSWQS

	001
	Oil and Grease
	---
	---
	15 mg/L
	15 mg/L
	PPL, TBEL

	001
	Temperature ˚F
	---
	90
	Report
	Report
	PPL, MSWQS

	001
	BOD5
	---
	---
	Report
	Report
	PPL, TJ

	001
	Zinc, Total Recoverable
	---
	0.065 mg/L
	0.0636 mg/L
	0.0636 mg/L
	PPL, TJ

	001
	TSS
	---
	---
	45 mg/L
	45 mg/L
	PPL, TJ

	001
	Ammonia (as N)
	---
	---
	Report
	Report
	PPL, TJ


   1 MSWQS = Mississippi Water Quality Standards, TBEL = Technology Based Effluent Limits, TJ = Technical Judgment

Flow shall be monitored monthly via instantaneous sampling. pH, Oil and Grease, BOD5, Zinc (TR), and Temperature shall be monitored monthly via grab sampling. TSS and Ammonia (as N) shall be monitored semi-annually via grab sampling. 

TSS and Ammonia (as N) DMRs shall be submitted annually; all other parameters shall submit DMRs quarterly. 
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