PERMIT RATIONALE FOR REISSUANCE
Illinois Central Railroad Company CN, McComb Yard
Pike County
McComb, Mississippi
Water NPDES No. MS0000141
July 16, 2026

I. FACILITY INFORMATION

Facility Name: 	Illinois Central Railroad Company CN, McComb Yard
Facility Address: 	South Railroad Ave
	McComb, MS  39648    
Jackson, 
Permit No.: 		MS0000141
SIC: 			4011
Permit Writer:  	Tye Gardner
EPD Branch:  		Water I Branch

II. NATURE OF BUSINESS

Railroad and Line Haul Operations. This facility is classified as an NPDES Minor Source.

III. EFFLUENT AND RECEIVING STREAM FLOW DATA

Effluent from Outfall 001 consists of treated storm water runoff from the facility storm water collection system, wash water from the locomotive refueling and maintenance apron, and storm water runoff from the railcar inspection and repair area. The outfall has a maximum daily flow of 0.003 MGD and will discharge directly into Town Creek (7Q10 flow = 0.2585 MGD) then into the Little Tangipahoa River located in the South Independent Streams Basin.

IV. 303(d) and TOTAL MAXIMUM DAILY LOAD (TMDL) ISSUES

Town Creek does not appear on the 2026 303(d) List of Impaired Water Bodies. 
The facility complies with the following applicable TMDLs: 

· Fecal Coliform – Tangipahoa River – Pike & Amite Counties – December 1999 – ID: 699121503 
· Organic Enrichment/Low Dissolved Oxygen & Total Ammonia Nitrogen – Little Tangipahoa River – Pike County – June 2004 – ID: 699121502 





V. TYPE OF WASTEWATER TREATMENT

· Oil/Water Separator 
· WW Lagoon #1 – Oil Separation and removal, solids settlement 
· WW Lagoon #2 – Flow Equalization and biological stabilization 

VI. EPA APPLICABLE CATEGORICAL GUIDELINES

None.

VII.	DATA FROM APPLICATION FORM (2C)




VIII. 	WATER QUALITY LIMITATIONS BASED ON WASTELOAD ALLOCATION 

	None.

1. CATEGORICAL GUIDELINE LIMITATIONS CALCULATIONS

Not Applicable.

TOXICITY SCREENING

Not Applicable.














XI.	PROPOSED FINAL LIMITATIONS 

1. Average Permit Limitations

	Outfall
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	[1]Basis

	001
	Flow (MGD)
	--
	--
	Report
	Report
	TJ, PPL

	001
	Oil and Grease
	--
	--
	10 mg/L
	10 mg/L
	TJ, PPL

	001
	pH
	--
	6.0 SU
	6.0 SU
	6.0 SU
	MSWQS




2. Maximum Permit Limitations

	Outfall
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	[1]Basis

	001
	Flow (MGD)
	--
	--
	Report
	Report
	TJ, PPL

	001
	Oil and Grease
	--
	--
	15 mg/L
	15 mg/L
	TJ, PPL

	001
	pH
	--
	9.0 SU
	9.0 SU
	9.0 SU
	MSWQS


 1Basis: MSWQS = Mississippi Water Quality Standards, PPL=Previous Permit Limits, TJ=Technical Judgment.



Flow shall be monitored monthly via instantaneous sampling; all other parameters shall be monitored monthly via grab sampling. 

All parameters’ DMRs shall be submitted quarterly. 
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Max. Daily Long Term Avg. No. of 

Value Value Analysis

BOD 11.7 mg/L --- 1

COD 18 mg/L --- 1

TOC 3.5 mg/L --- 1

TSS 3.3 mg/L --- 1

Ammonia  (as N) <0.1 mg/L --- 1

Flow (MGD) 0.003 MGD --- Totalizer

Temperature (winter) Ambient --- ---

Temperature (summer) Ambient --- ---

pH (SU) 9 (max) --- 18

Oil and grease 6.1 mg/L 0.246 mg/L 18
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				Max. Daily		Long Term Avg.		No. of 

				Value		Value		Analysis

		BOD		11.7 mg/L		---		1

		COD		18 mg/L		---		1

		TOC		3.5 mg/L		---		1

		TSS		3.3 mg/L		---		1

		Ammonia  (as N)		<0.1 mg/L		---		1

		Flow (MGD)		0.003 MGD		---		Totalizer

		Temperature (winter)		Ambient		---		---

		Temperature (summer)		Ambient		---		---

		pH (SU)		9 (max)		---		18

		Oil and grease		6.1 mg/L		0.246 mg/L		18












































































































