PUBLIC NOTICE PERMIT RATIONALE FOR REISSUANCE
Canton, City of, Canton Sanitary Landfill
Madison County
Canton, Mississippi
Water NPDES No. MSS058548
July 13, 2026

I. FACILITY INFORMATION

Facility Name:		Canton, City of, Canton Sanitary Landfill
Facility Address:	303 Soldier Colony Road 
	Canton, MS  39046    
Canton, 
Permit No.:		MSS058548
SIC:			4953
Permit Writer:		Rusty Parrish
EPD Branch:		Water II Branch

II. NATURE OF BUSINESS

Municipal Solid Waste Landfill.

III. EFFLUENT AND RECEIVING STREAM FLOW DATA

	Outfall No.
	Permitting Status
	Total Area Drained
	Construction Status

	001
	Currently permitted
	Approximately 52.0 acres
	Constructed

	002
	Currently permitted
	Approximately 31.0 acres
	Constructed

	003
	Currently permitted
	Approximately 18.0 acres
	Constructed

	004
	Proposed
	Approximately 45.0 acres
	Not Constructed



Discharges from all four outfalls consist of storm water runoff associated with the construction, development, and operation of the municipal landfill, except for working face runoff and leachate. Outfalls 001, 002, and 003 currently discharge into Bear Creek. Outfall 004 will discharge into Bear Creek. Bear Creek is located in the Big Black River Basin.

IV. 303(d) and TMDL ISSUES

Bear Creek is on the Mississippi 2024 List of Impaired Water Bodies. The proposed permit complies with the following TMDLs:
· Sediment – Lower Big Black River – Big Black River Basin – January 2007 – ID: 107012603
· Nutrients and Organic Enrichment/ Low DO – Bear Creek & Tilda Bogue – Hinds & Madison Counties – October 2009
· Sediment – Big Black River Watershed – Big Black River Basin – January 2007 – ID: 107012601
· DDT & Toxaphene – Big Black & Tombigbee River Basins – November 2005 – ID: 105111401
· Fecal Coliform – Big Black River Basin Segment 2 – Warren County – October 24, 2000
· pH – Big Black River Watershed – Hinds & Warren Counties – January 2018

V. TYPE OF WASTEWATER TREATMENT:

Stormwater is stored in sedimentation basins.

VI. EPA APPLICABLE CATEGORICAL GUIDELINES

Not applicable.

DATA FROM APPLICATION FORM 2F

	Outfall 001

	Parameter
	Maximum Daily Value
	Average Daily Value

	Oil and Grease
	Data Unavailable
	Data Unavailable

	Biochemical Oxygen Demand (BOD5)
	BDL*
	BDL*

	Chemical Oxygen Demand (COD)
	43 mg/L
	43 mg/L

	Total Suspended Solids (TSS)
	88 mg/L
	88 mg/L

	Total Phosphorus
	Data Unavailable
	Data Unavailable

	Total Kjeldahl Nitrogen (TKN)
	Data Unavailable
	Data Unavailable

	Total Nitrogen (as N)
	Data Unavailable
	Data Unavailable

	pH (minimum)
	7.8 SU
	7.8 SU

	pH (maximum)
	7.8 SU
	7.8 SU

	Turbidity
	84.3 NTU
	84.3 NTU



	Outfall 002

	Parameter
	Maximum Daily Value
	Average Daily Value

	Oil and Grease
	Data Unavailable
	Data Unavailable

	Biochemical Oxygen Demand (BOD5)
	BDL*
	BDL*

	Chemical Oxygen Demand (COD)
	42 mg/L
	42 mg/L

	Total Suspended Solids (TSS)
	8 mg/L
	8 mg/L

	Total Phosphorus
	Data Unavailable
	Data Unavailable

	Total Kjeldahl Nitrogen (TKN)
	Data Unavailable
	Data Unavailable

	Total Nitrogen (as N)
	Data Unavailable
	Data Unavailable

	pH (minimum)
	7.9 SU
	7.9 SU

	pH (maximum)
	7.9 SU
	7.9 SU

	Turbidity
	9.1 NTU
	9.1 NTU





	Outfall 003

	Parameter
	Maximum Daily Value
	Average Daily Value

	Oil and Grease
	Data Unavailable
	Data Unavailable

	Biochemical Oxygen Demand (BOD5)
	BDL*
	BDL*

	Chemical Oxygen Demand (COD)
	42 mg/L
	42 mg/L

	Total Suspended Solids (TSS)
	8 mg/L
	8 mg/L

	Total Phosphorus
	Data Unavailable
	Data Unavailable

	Total Kjeldahl Nitrogen (TKN)
	Data Unavailable
	Data Unavailable

	Total Nitrogen (as N)
	Data Unavailable
	Data Unavailable

	pH (minimum)
	7.9 SU
	7.9 SU

	pH (maximum)
	7.9 SU
	7.9 SU

	Turbidity
	9.7 NTU
	9.7 NTU



	Outfall 004

	Parameter
	Maximum Daily Value
	Average Daily Value

	Oil and Grease
	Data Unavailable
	Data Unavailable

	Biochemical Oxygen Demand (BOD5)
	BDL*
	BDL*

	Chemical Oxygen Demand (COD)
	42 mg/L
	42 mg/L

	Total Suspended Solids (TSS)
	35 mg/L
	35 mg/L

	Total Phosphorus
	Data Unavailable
	Data Unavailable

	Total Kjeldahl Nitrogen (TKN)
	Data Unavailable
	Data Unavailable

	Total Nitrogen (as N)
	Data Unavailable
	Data Unavailable

	pH (minimum)
	7.9 SU
	7.9 SU

	pH (maximum)
	7.9 SU
	7.9 SU

	Turbidity
	34.4 NTU
	34.4 NTU


*BDL = Below Detection Limit

Data for Outfall 004 is an average of existing Outfalls 001, 002, and 003.

PROPOSED FINAL LIMITATIONS 

1. Average Permit Limitations

	Outfalls
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation (PPL)
	Proposed Permit Limitation
	Basis1

	001, 002, 003, & 004
	COD
	None
	None
	Report
	Report
	PPL

	
	BOD5
	None
	None
	Report
	Report
	PPL

	
	pH
	None
	None
	6.0 SU
	6.0 SU
	MSWQS

	
	TSS
	None
	None
	90 mg/L
	90 mg/L
	PPL

	
	Turbidity
	None
	None
	Report
	Report
	PPL



2. 
Maximum Permit Limitations

	Outfalls
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation (PPL)
	Proposed Permit Limitation
	Basis1

	001, 002, 003, & 004
	COD
	None
	None
	Report
	Report
	PPL

	
	Flow
	None
	None
	Report
	Report
	PPL

	
	BOD5
	None
	None
	Report
	Report
	PPL

	
	pH
	None
	None
	9.0 SU
	9.0 SU
	MSWQS

	
	TSS
	None
	None
	Report
	Report
	PPL

	
	Turbidity
	None
	None
	Report
	Report
	PPL


1Basis: PPL = Present Permit Limitation; MSWQS = Mississippi Water Quality Standard; SLL = Standard Landfill Limitation

The parameters shall be monitored monthly via grab sampling. Results will be reported quarterly (January, April, July, and October) on Discharge Monitoring Reports (DMRs).

An Antidegradation Report was submitted on April 26, 2024. MDEQ completed the review and had no comments.

The Stormwater Pollution Prevention Plan (SWPPP) submitted by the facility in October 2023 meets the current SWPPP conditions of the permit.
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