PERMIT RATIONALE FOR REISSUANCE
ANR Pipeline Company, Greenville Compressor Station
Washington County
Greenville, Mississippi
Water NPDES No. MS0048216
July 16, 2026

I. FACILITY INFORMATION

Facility Name:		ANR Pipeline Company, Greenville Compressor Station
Facility Address: 	1336 South Raceway Road 
	Greenville, MS  38704    
Greenville, 
Permit No.: 		MS0048216
SIC: 			4922
Permit Writer: 	Tye Gardner
EPD Branch: 		Water I Branch 

II. NATURE OF BUSINESS

ANR Pipeline Company is an interstate transmission company that transports natural gas through a series of subsurface pipelines and compressor stations. Natural gas is moved from productions areas to customers located throughout the United States.  This facility is classified as an NPDES Minor Source.

III. EFFLUENT AND RECEIVING STREAM FLOW DATA

[bookmark: Text2]Outfall 001:   The facility wastewater consists of storm water from downspouts, paved areas, fin fan area, diked tank area, floor wash water, equipment wash water, and compressor condensate. All of the process water passes through an oil/water separator. All water flows through a retention pond on the southwest corner of the property and discharges via Outfall 001. The wastewater leaves the property and enters a roadside ditch and thence to Main Canal. This outfall has a long-term average daily discharge of 0.00195 MGD and is located in the Yazoo River Basin.

IV. 303(d) and TOTAL MAXIMUM DAILY LOAD (TMDL) ISSUES

Main Canal does not appear on the 2026 303(d) List of Impaired Water Bodies. 
The facility complies with the following applicable TMDLs: 

· Organic Enrichment/Low DO and Nutrients – Black Bayou – Washington & Bolivar Counties – June 2003 – ID: 903063004 
· Total Nitrogen & Total Phosphorus – Yazoo River Basin – June 2008 – ID: 908063054 
· Sediment – Steele Bayou Watershed including Main Canal, Granny Baker Bayou, Granicus Bayou, and Black Bayou – Yazoo River Basin – June 2003 – ID: 903063015 
· Organic Enrichment/Low DO – Swiftwater Bayou Watershed – Washington County – February 2014 
· Legacy Pesticides DDT and Toxaphene – Yazoo River Basin – May 2003 – ID: 903051601 
· Legacy Pesticides DDT and Toxaphene – Yazoo River Basin – November 2005 – ID: 905110401
· Sediment – Yazoo River Basin Delta Region – April 2008 – ID: 908041702 

V. TYPE OF WASTEWATER TREATMENT

Carbon filtration, organoclay filtration, bag filtration, oil/water separation, sedimentation, evaporation, and discharge to surface water.

VI. EPA APPLICABLE CATEGORICAL GUIDELINES

Not Applicable.

VII.	DATA FROM APPLICATION FORM (2C)

	Parameter
	Maximum Daily Value

	BOD
	8.1 mg/l

	COD
	20 mg/l

	TOC
	1.1 mg/l

	Total Suspended Solid
	<8.0 mg/l

	Ammonia
	2.4 mg/l

	Temperature (Winter)
	22.28 ºC

	Temperature (Summer)
	24.56 ºC

	pH
	8.30 (max) SU

	Arsenic, Total
	0.0019 mg/l

	Cadmium, Total
	<0.00050 mg/l

	Chromium, Total
	<2.0 mg/l

	Lead, Total
	<0.0050 mg/l

	Mercury, Total
	<0.00020 mg/l

	Oil and Grease
	2.87 mg/l

	PCB-1242
	<0.00010 mg/l

	PCB-1254
	<0.00010 mg/l

	PCB-1221
	<0.00010 mg/l

	PCB-1232
	<0.00010 mg/l

	PCB-1248
	<0.00010 mg/l

	PCB-1260
	<0.00010 mg/l

	PCB-1016
	<0.00010 mg/l

	Barium, Total
	0.0300 mg/l

	Ethylene glycol
	<100 mg/l




VIII. 	WATER QUALITY LIMITATIONS BASED ON WASTELOAD ALLOCATION 
	
	Not Applicable.

1. CATEGORICAL GUIDELINE LIMITATIONS CALCULATIONS

Not Applicable.

TOXICITY SCREENING

Not Applicable.

XI.	PROPOSED FINAL LIMITATIONS 

1. Average Permit Limitations

	Outfalls
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	[1]Basis

	001
	Flow (MGD)
	--
	--
	Report
	Report
	TJ, PPL

	001
	Oil and Grease
	--
	--
	10 mg/L
	10 mg/L
	TJ, PPL

	001
	pH
	--
	6.0 SU
	6.0 SU
	6.0 SU
	MSWQS




2. Maximum Permit Limitations

	Outfalls
	Parameter
	Categorical Limitation
	Water Quality Limitation
	Present Permit Limitation
	Proposed Permit Limitation
	[1]Basis

	001
	Flow (MGD)
	--
	--
	Report
	Report
	TJ, PPL

	001
	Oil and Grease
	--
	--
	15 mg/L
	15 mg/L
	TJ, PPL

	001
	pH
	--
	9.0 SU
	9.0 SU
	9.0 SU
	MSWQS

	001
	Temperature ˚F
	--
	90 ˚F
	 90 ˚F
	 90 ˚F
	MSWQS


      1Basis: MSWQS = Mississippi Water Quality Standards, PPL=Previous Permit Limits, TJ=Technical Judgment.

Flow and Temperature shall be monitored monthly via instantaneous sampling. pH and Oil & Grease shall be monitored monthly via grab sampling. 

All parameters’ DMRs shall be submitted quarterly.
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