PERMIT RATIONALE FOR REISSUANCE
MS District UPC Camp Grounds
Hinds County
Raymond, Mississippi
Water NPDES No. MS0031186
June 3, 2021

I.	CLASSIFICATION - Commercial

II.	DESCRIPTION OF WASTEWATER - Domestic

III.	DESCRIPTION OF WASTEWATER TREATMENT – Domestic wastewater from the Pentecostal Campground is collected and treated through a conventional lagoon.

IV.	RECEIVING WATERS – Unnamed creek thence Baker’s Creek.  Baker’s Creek does appear on the current State of Mississippi 303(d) List of Impaired Waterbodies for biological impairment.  A TMDL for biological impairment due to nutrients and organic enrichment/ low dissolved oxygen for Bakers Creek. All the limitations complies with the TMDL. Baker’s Creek is in the Big Black River drainage basin.  Baker’s Creek is classified as Fish and Wildlife. 

V.	APPLICABLE GUIDELINES – State of Mississippi Wastewater Regulations (11 MS admin code part 6), State of Mississippi Water Quality Criteria (11 MS admin code part 6), Commercial Facility Guidelines, Total Maximum Daily Load (TMDL).

VI.	SUMMARY OF DISCHARGE LIMITATIONS – 

Parameter		Value					Basis
Flow			0.015 MGD			Design
BOD			30 mg/l				Commercial Guidelines
TSS			90 mg/l 				Technology
E. coli			126 Col. /100 ml		Commercial Guidelines
Chlorine		0.1 to 1.0 mg/l		Commercial Guidelines
Ammonia Nitrogen	2.0 mg/l				TMDL
Total Phosphorus	0.65 lbs/day		TMDL
Total Nitrogen		1.44 lbs/day		TMDL
pH			6.0 to 9.0 S.U.		11 MS admin part 6