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INFORMATION RELATIVE TO 
THE TITLE V OPERATING PERMIT
[Insert Date]

GENERAL FACILITY INFORMATION
Facility Name:	Greenway Environmental Services, LLC (d.b.a. Green Meadow Sustainable Solutions)
Facility Address: 4451 Highway 61 North; Fayette, MS 39069
County: Jefferson
SIC Code(s): 4953 (Refuse Systems)
NAICS Code(s): 562212 (Solid Waste Landfills)

APPLICATION SUMMARY 
	Permit No.: 1320-00019
Permit Action: Renewal (w/Significant Modification)
Permit Folder: PER20160001
Application Receipt Date: February 2, 2016 (initial); January 3, 2021 (revised); September 9, 2025 (revised)
Application Deemed Complete: August 10, 2016
CBI Submitted?: No
	NSPS (Part 60): XXX
NESHAP (Part 61): M
NESHAP (Part 63): N/A
112(r) / RMP: N/A
Other: N/A



FACILITY DESCRIPTION
Greenway Environmental Services, LLC (doing business as Green Meadow Sustainable Solutions) (“Greenway”) is an existing municipal solid waste (MSW) landfill that accepts non-hazardous solid waste from residential, industrial, and institutional sources (which includes – but not limited to – household waste, commercial waste, and industrial waste, rubbish, construction debris, and demolition material).  On November 3, 2020, the MSW landfill was purchased by Greenway from Riverbend Environmental Services, LLC (“Riverbend”).

The overall landfill consists of an approximately 160.4-acre waste footprint with twelve (12) potential new cells and seven (7) existing / active cells for a total capacity of approximately 23,557,000 cubic yards (or 18,845,600 tons – approximately 17,096,441 megagrams).

TITLE V SOURCE APPLICABILITY 
Pursuant to 40 CFR Part 60 – Subpart XXX [specifically 40 CFR 60.762(b) and (c)], Greenway is required to obtain a Title V Operating Permit (TVOP) given that the MSW landfill has a design capacity equal to / greater than 2.5 million megagrams (or 2,755,778 tons) and 2.5 million cubic meters (or 326,988 cubic yards).

Regarding air emissions, the facility’s potential-to-emit (PTE) does not the Title V major source threshold of 100 tons per year (tpy) for any of the applicable criteria air pollutants.  In addition, the facility’s potential-to-emit hazardous air pollutants (HAPs) does not exceed the major source threshold of 25 tons per year for all HAPs in total or 10 tons per year for each individual HAP.  Therefore, the facility is considered an area source for HAPs.

Facility-Wide Potential-to-Emit Summary1
	Pollutant
	PTE Emissions
(tons/yr)

	Particulate Matter (TSP)
	4.87

	PM10
	1.25

	PM2.5
	0.17

	Sulfur Dioxide (SO2)
	--

	Nitrogen Oxides (NOx)
	--

	Carbon Monoxide (CO)
	3.98

	Volatile Organic Compounds (VOCs)
	16.11

	Total Reduced Sulfur (TRS)
	1.86

	Lead
	--

	CFC/HCFC
	--

	Total HAPs
	9.1


1 The PTE emissions reflect any emission limits or enforceable restrictions included in the proposed permit.

PREVENTION OF SIGNIFICANT DETERIORATION (PSD) APPLICABILITY
A MSW landfill is not one of the 28 categorical facilities listed in 40 CFR 52.21(b)(1)(i)(A); therefore, the applicable PSD major source threshold is 250 tons per year for each regulated New Source Review (NSR) pollutant (with fugitive emissions not included in the initial assessment).  Based on the emissions profile, Greenway does not have the potential to emit any regulated pollutant more than 250 tons per year.  Therefore, the facility is considered an existing “minor NSR source” under the PSD program.

This permitting action will not change the current PSD status of the facility.

FACILITY MODIFICATIONS AND/OR PERMIT CHANGES
On February 2, 2016, Riverbend submitted an application requesting a renewal of the TVOP issued August 9, 2011.  Upon preliminary review of the application, MDEQ staff transmitted a Notice of Deficiency to the facility on April 6, 2016, that outlined several deficiencies (primarily missing information).  Accordingly, Riverbend submitted a revised application that addressed all indicated deficiencies on July 27, 2016.  Within the overall application, Riverbend outlined that the design capacity of the landfill would remain unchanged (i.e., 9,933,675 megagrams).  

On January 3, 2021, Greenway submitted a revised application to reflect their acquisition of the MSW landfill from Riverbend.

On September 9, 2025, Greenway submitted an updated revised application to include the proposed “expansion” of the landfill’s design capacity from 9,933,675 megagrams to 17,096,441 megagrams with the inclusion of twelve (12) additional cells (for solid waste regulatory purposes, the mentioned twelve (12) cells have always been considered part of the overall 160.4-acre footprint) and to formally clarify that the facility no longer has non-road stationary internal combustion engines on-site for emergency power generation.  

Despite the increase in design capacity, Greenway conveyed that the generation of non-methane organic compounds (NMOCs) – from waste degradation – has not exceeded the Federal regulatory threshold of 34 megagrams per year.  As such, the facility has not employed an active gas collection and control system (GCCS).

As part of this proposed renewal permitting action, MDEQ is also addressing the following 502(b)(10) changes:

· March 22, 2012: Riverbend (the owner at the time) incorporated a solidification process.  This process utilizes bulking agents to solidify liquids and semi-liquids for adequate placement within the landfill.

· March 13, 2024: Greenway installed and commenced continuous operation of a 5.5 MMBTU per hour natural gas-fired flare to minimize odor from landfill gas passively venting to the atmosphere.  Based on additional information by Greenway, the denoted flare combust gas specifically captured from Cell 1-5.

· June 14, 2024: Greenway installed and commenced continuous operation of two (2) 5.5 MMBTU per hour natural gas-fired flares to minimize odor from landfill gas passively venting to the atmosphere.  The denoted flare combust gas respectively captured from Cells 1-4A and 1-4C.  While the document only denotes the installation and operation of one (1) flare, additional information received June 26, 2026 clarifies that original proposed change encompassed two (2) flares.

COMPLIANCE ASSURANCE MONITORING (CAM) APPLICABILITY
40 CFR Part 64 specifies the requirements for CAM.  The general applicability of this rule can be found in 40 CFR 64.2 and requires a Title V source to comply with the CAM requirements if all three of the following criteria are met for a pollutant-specific emission unit (PSEU):

1. The unit is subject to an emission limitation or standard for a regulated air pollutant other than exemptions under 40 CFR 64.2(b)(1);

2. The unit uses a control device to comply with the standard; and

3. The unit has pre-control emissions exceeding Title V major source threshold.

As the MSW landfill (i.e., the PSEU) is not subject to an emission limit that meets the indicated criteria nor is there any control equipment associated with the landfill, CAM is not applicable.

NATIONAL EMISSION STANDARDS FOR HAZARDOUS AIR POLLUTANTS (NESHAP) APPLICABILITY
40 CFR Part 61, Subpart M –National Emission Standards for Asbestos:  The provisions of Subpart M are applicable to an active waste disposal site that receives asbestos-containing materials for final disposal from sources also applicable to Subpart M.  Given that Greenway has denoted that it will accept waste that asbestos-containing material, the landfill is subject to Subpart M.

40 CFR Part 63, Subpart AAAA – NESHAP: Municipal Solid Waste Landfills:  The provisions of Subpart AAAA are applicable to a municipal solid waste (MSW) landfill that has accepted waste since November 8, 1987, has additional capacity for waste deposition, and meets any one of the three following criteria:
1. The MSW landfill is a major source of HAPs as defined in 40 CFR 63.2, Subpart A; 
2. The MSW landfill is collocated with a major source as defined in 40 CFR 63.2, Subpart A; or
3. The MSW landfill is an area source that has a design capacity equal to / greater than 2.5 megagrams and 2.5 million cubic meters and has an estimated uncontrolled emissions equal to / greater than 50 megagrams of NMOCs per year as calculated in accordance with the subpart.

The landfill is considered an area source for HAPs (based on its potential-to-emit emissions profile) and not collocated with another source that could be considered HAP major source.  In addition, while the landfill is an area source and has a design capacity that exceeds the referenced thresholds (for mass and volume), it does not have the capability to generate uncontrolled emissions equal to / greater than 50 megagrams of NMOCs per year (40 CFR Part 60, Subpart XXX restricts a landfill’s potential-to-emit NMOCs uncontrolled to no more than 34 megagrams per year before the facility must install a GCCS).  Therefore, Greenway is not subject to Subpart AAAA.

NEW SOURCE PERFORMANCE STANDARDS (NSPS) APPLICABILITY
40 CFR Part 60, Subpart Cf – Emission Guidelines and Compliance Times for Municipal Solid Waste Landfills:  The provisions of Subpart Cf apply to any MSW landfill that commenced construction, modification, or reconstruction on or before July 17, 2014.  However, as an “emissions guideline”, a facility only becomes subject to Subpart Cf once the applicable environmental permit regulatory authority receives delegated authority through EPA’s approval of a State Plan completed in accordance with 40 CFR Part 60, Subpart Ba (Adoption and Submittal of State Plans for Designated Facilities).  

While MDEQ has not received delegated authority of Subpart Cf, Greenway has stated construction of the proposed “expansion” will commence upon issuance of this renewed TVOP (along with the renewed solid waste permit).  As construction of the denoted expansion will be considered a “modification” (as defined by 40 CFR Part 60, Subpart XXX), Greenway will not be subject to Subpart Cf.

40 CFR Part 60, Subpart XXX – Standards of Performance for Municipal Solid Waste Landfills that Commenced Construction, Reconstruction, or Modification after July 17, 2014:  The provisions of Subpart XXX apply to any MSW landfill that commenced construction, reconstruction, or modification after July 17, 22014.  As construction of the denoted expansion will be considered a “modification” and will occur after the indicated “date of applicability”, Greenway will be subject to Subpart Cf upon issuance of this renewed TVOP.

FEDERAL PLAN
40 CFR Part 62, Subpart OOO – Federal Plan Requirements for Municipal Solid Waste Landfills That Commenced Construction On or Before July 17, 2014 and Have Not Been Modified or Reconstructed Since July 17, 2014:  The provisions of the Federal Plan implementing the 2016 Emission Guidelines and Compliance Times for Existing Municipal Solid Waste Landfills (i.e., 40 CFR 60 Subpart Cf) was finalized on May 10, 2021. Since MDEQ does not have an approved State Plan, the Federal Plan found in 40 CFR Part 62 – Subpart OOO is in effect and strictly enforced by EPA Region 4. 

As Greenway has stated construction of the proposed “expansion” will commence upon issuance of this renewed TVOP (along with the renewed solid waste permit).  As construction of the denoted expansion will be considered a “modification” (as defined by 40 CFR Part 60, Subpart XXX), Greenway will not be subject to the Federal Plan given the non-applicability to Subpart Cf.

SPECIFIC APPLICABLE REQUIREMENTS

	Emission Point No.
	Pollutant
	Draft Permit Emission Limits
	Monitoring Requirements

	AA-001
	NMOCs
	34 Mg / Year
(threshold for GCCS)
	Calculate emissions in accordance with the applicable “Tier” on either an annual basis or on a 5-year estimation.



OTHER REQUIREMENTS:
N/A


[bookmark: aiid]10186 PER20160001		
